         

Résumé        
         Des essais préliminaires de dépôts de films de zéolithes sur un support métallique ont été réalisés dans ce présent mémoire. Des zéolithes de types ZSM-5 ont été obtenues par élaboration hydrothermale et déposées par voie in situ sur un alliage d’aluminium. Le processus d’élaboration et de dépôt de zéolithes a été réalisé dans un autoclave en Téflon pendant un temps de chauffage de 24 h à 170°C et sous pression autogène. Après dépôt, les différents revêtements obtenus ont fait l'objet d'une caractérisation par différentes techniques à savoir, la (DRX, ATG/ATD, (EDS). Les tests préliminaires et les résultats obtenus montrent que le revêtement de l’alliage d’aluminium par un ou plusieurs films de zéolithes est possible.

Abstract
        Preliminary tests of zeolite film coatings on a metal support were carried out in this present work. ZSM-5 zeolites were obtained by hydrothermal synthesis and were deposited by in situ way on an aluminium alloy. The synthesis process and coating zeolites were carried out in a Teflon autoclave during 24 H in 170°C and under autogenously pressure. These zeolites were characterized by various techniques as X ray diffraction, gravimetric and differential thermal analysis (TGA/DTA), infra-red spectroscopy and electronic scanning microscopy as well as the spectroscopy of dispersive energy (EDS). The preliminary tests and the results obtained show that the coating of aluminium alloy by one or more films of zeolites is possible.

