Résumé : 
       Ce travail à pour objectif de contribuer à l’approfondissent et à l’amélioration des  connaissances du pouvoir d’élimination des orthophosphates par les résidus d’incinération de produits pharmaceutiques périmés. L’étude en batch a montré la quantité adsorbée dépend de plusieurs paramètres à savoir : du pH, de la température, de la concentration de l’adsorbant et de la concentration initiale des orthophosphates.  Les résultats des isothermes d’adsorption favorisent l’isotherme de Freundlich pour étant la plus appropriée à décrire le phénomène d’adsorption. Enfin et pour conclure, la méthode des plans d’expérience a permis d’établir et de mettre au point un modèle mathématique quantifiant l’influence de chaque paramètre sur le rendement d’adsorption des  orthophosphates .
Abstract:
        This work aims to contribute to the deepening and improving knowledge of the power of removal of orthophosphate by incineration residues expired pharmaceuticals. The batch study show that the amount adsorbed depends on several parameters and namely: the pH, temperature, concentration of adsorbent and initial concentration of orthophosphate. The results of adsorption isotherms favor the Freundlich isotherm to be the most appropriate to describe the adsorption. Finally and to conclude, the experimental designs helped to establish and develop a mathematical model quantifying, the influence of each parameter on the adsorption of orthophosphate performance.
